CAN-200: Значения скорости обмена по шине CAN

CAN-200 1.3.1

Макросы
Значения скорости обмена по шине CAN

## Макросы

#define | CAN_SPEED_USER_DEFINED(btr0, btr1) (0xffff | (((btr0) & 0xff) << 24) | (((btr1) & 0xff) << 16))
| Скорость определенная пользователем
#define | IS_CAN_SPEED_USER_DEFINED(speed) ((0xffff == ((speed) & 0xffff)) ? 1 : 0)
| 1 - скорость определяемая пользователем, 0 - одна из стандартных скоростей
#define | CAN_SPEED_GET_BTR0(speed) (((speed) >> 24) & 0xff)
| Возвращает значение регсистра BTR0 для скоростей задаваемых пользователем
#define | CAN_SPEED_GET_BTR1(speed) (((speed) >> 16) & 0xff)
| Возвращает значение регсистра BTR1 для скоростей задаваемых пользователем
#define | CAN_SPEED_1000 1000
| Скорость 1 Mbit/sec.
#define | CAN_SPEED_800 800
| Скорость 800 kbit/sec.
#define | CAN_SPEED_500 500
| Скорость 500 kbit/sec.
#define | CAN_SPEED_250 250
| Скорость 250 kbit/sec.
#define | CAN_SPEED_125 125
| Скорость 125 kbit/sec.
#define | CAN_SPEED_50 50
| Скорость 50 kbit/sec.
#define | CAN_SPEED_20 20
| Скорость 20 kbit/sec.
#define | CAN_SPEED_10 10
| Скорость 10 kbit/sec.

## Подробное описание

CAN-200 documentation. Copyright (c) 2012 - 2017 Elcus Corporation. All rights reserved.