Monitor for ELCUS C167M-3U v2.x Board
(monitor version: 1.1)

You need under Options - L166 Misc RESERVE:
  8H-0BH, 140H-143H

Memory map:
 00:0000h - 00:65FFh  free SRAM (32 KBytes, CS0 connected)
 00:6600h - 00:7FFFh  SRAM for monitor code, data and interrupt table (32 KBytes, CS0 connected)
 00:8000h - 00:FFFFh  on-chip RAM and SFR's
 01:0000h - 01:0FFFh  TAM1-ISA/TXM1-ISA registers (4 KBytes, CS2 connected)
 08:0000h - 0F:FFFFh  free MRAM (512KBytes, CS1 connected)
 20:0000h - 20:BFFFh  MultiCAN, USIC0-3 registers
 C0:0000h - D8:FFFFh  on-chip flash memory (1600 KBytes)
 E0:0000h - E1:BFFFh  on-chip PSRAM memory (112 KBytes)


